NIRSPEC

UCLA Astrophysics Program	U.C. Berkeley	W.M.Keck Observatory

George Brims	October 12, 1995

NIRSPEC Cryomechanics Design Note 06.00

Window mount

Introduction

The window mount might seem to be a very simple thing to have a design document of its own, but the walls of the vacuum enclosure are going to distort a lot, so we need to take this into account when designing the mount for the window.

What next?

The design of the vacuum enclosure needs to be completed, so that we can then produce a design for the window mount that will avoid problems with aligning the instrument to the telescope.